; Local-only override (gitignored) pointing the Heltec V3 observer env at a custom
; framework whose mbedTLS archives were rebuilt with an asymmetric TLS record buffer:
;   CONFIG_MBEDTLS_ASYMMETRIC_CONTENT_LEN=y
;   CONFIG_MBEDTLS_SSL_IN_CONTENT_LEN=16384   (unchanged — a peer may send a 16 KiB record)
;   CONFIG_MBEDTLS_SSL_OUT_CONTENT_LEN=4096   (was 16384)
;
; Expected: ~12 KiB less internal DRAM per TLS connection, ~24 KiB across two broker slots.
; Built from the shipped sdkconfig verbatim plus those three lines, so the archives differ
; only by this change. See docs/mbedtls-tls-footprint.md.
;
; Absolute path, hence local-only: not committable.

[env:Heltec_v3_repeater_observer_mqtt]
platform_packages =
  framework-arduinoespressif32 @ file:///Users/adam/framework-arduinoespressif32-tlsfix
