# eturnal TURN server - Synapse

## Keyboard shortcuts

Press `←` or `→` to navigate between chapters

Press `S` or `/` to search in the book

Press `?` to show this help

Press `Esc` to hide this help

# eturnal TURN server

The following sections describe how to install eturnal (which implements the TURN REST API).

## `eturnal` setup

### Initial installation

The `eturnal` TURN server implementation is available from a variety of sources such as native package managers, binary packages, installation from source or container image. They are all described here.

Quick-Test instructions in a Linux Shell or with Docker are available as well.

### Configuration

After installation, `eturnal` usually ships a default configuration file here: `/etc/eturnal.yml` (and, if not found there, there is a backup file here: `/opt/eturnal/etc/eturnal.yml`). It uses the (indentation-sensitive!) YAML format. The file contains further explanations.

Here are some hints how to configure eturnal on your host machine or when using e.g. Docker. You may also further deep dive into the reference documentation.

`eturnal` runs out of the box with the default configuration. To enable TURN and to integrate it with your homeserver, some aspects in `eturnal`’s default configuration file must be edited:

1. Homeserver’s `turn_shared_secret` and eturnal’s shared `secret` for authentication

   Both need to have the same value. Uncomment and adjust this line in `eturnal`’s configuration file:

       secret: "long-and-cryptic"     # Shared secret, CHANGE THIS.

   One way to generate a `secret` is with `pwgen`:

       pwgen -s 64 1

2. Public IP address

   If your TURN server is behind NAT, the NAT gateway must have an external, publicly-reachable IP address. `eturnal` tries to autodetect the public IP address, however, it may also be configured by uncommenting and adjusting this line, so `eturnal` advertises that address to connecting clients:

       relay_ipv4_addr: "203.0.113.4" # The server's public IPv4 address.

   If your NAT gateway is reachable over both IPv4 and IPv6, you may configure `eturnal` to advertise each available address:

       relay_ipv4_addr: "203.0.113.4" # The server's public IPv4 address.
       relay_ipv6_addr: "2001:db8::4" # The server's public IPv6 address (optional).

   When advertising an external IPv6 address, ensure that the firewall and network settings of the system running your TURN server are configured to accept IPv6 traffic, and that the TURN server is listening on the local IPv6 address that is mapped by NAT to the external IPv6 address.

3. Logging

   If `eturnal` was started by systemd, log files are written into the `/var/log/eturnal` directory by default. In order to log to the journal instead, the `log_dir` option can be set to `stdout` in the configuration file.

4. Security considerations

   Consider your security settings. TURN lets users request a relay which will connect to arbitrary IP addresses and ports. The following configuration is suggested as a minimum starting point, see also the official documentation:

       ## Reject TURN relaying from/to the following addresses/networks:
       blacklist:                 # This is the default blacklist.
           - "127.0.0.0/8"        # IPv4 loopback.
           - "::1"                # IPv6 loopback.
           - recommended          # Expands to a number of networks recommended to be
                                  # blocked, but includes private networks. Those
                                  # would have to be 'whitelist'ed if eturnal serves
                                  # local clients/peers within such networks.

   To whitelist IP addresses or specific (private) networks, you need to add a whitelist part into the configuration file, e.g.:

       whitelist:
           - "192.168.0.0/16"
           - "203.0.113.113"
           - "2001:db8::/64"

   The more specific, the better.

5. TURNS (TURN via TLS/DTLS)

   Also consider supporting TLS/DTLS. To do this, adjust the following settings in the `eturnal.yml` configuration file (TLS parts should not be commented anymore):

       listen:
           - ip: "::"
             port: 3478
             transport: udp
           - ip: "::"
             port: 3478
             transport: tcp
           - ip: "::"
             port: 5349
             transport: tls

       ## TLS certificate/key files (must be readable by 'eturnal' user!):
       tls_crt_file: /etc/eturnal/tls/crt.pem
       tls_key_file: /etc/eturnal/tls/key.pem

   In this case, replace the `turn:` schemes in homeserver’s `turn_uris` settings with `turns:`. More is described here.

   We recommend that you only try to set up TLS/DTLS once you have set up a basic installation and got it working.

   NB: If your TLS certificate was provided by Let’s Encrypt, TLS/DTLS will not work with any Matrix client that uses Chromium’s WebRTC library. This currently includes Element Android & iOS; for more details, see their respective issues as well as the underlying WebRTC issue. Consider using a ZeroSSL certificate for your TURN server as a working alternative.

6. Firewall

   Ensure your firewall allows traffic into the TURN server on the ports you’ve configured it to listen on (By default: 3478 and 5349 for TURN traffic (remember to allow both TCP and UDP traffic), and ports 49152-65535 for the UDP relay.)

7. Reload/ restarting `eturnal`

   Changes in the configuration file require `eturnal` to reload/ restart, this can be achieved by:

       eturnalctl reload

   `eturnal` performs a configuration check before actually reloading/ restarting and provides hints, if something is not correctly configured.

### eturnalctl opterations script

`eturnal` offers a handy operations script which can be called e.g. to check, whether the service is up, to restart the service, to query how many active sessions exist, to change logging behaviour and so on.

Hint: If `eturnalctl` is not part of your `$PATH`, consider either sym-linking it (e.g. ´ln -s /opt/eturnal/bin/eturnalctl /usr/local/bin/eturnalctl´) or call it from the default `eturnal` directory directly: e.g. `/opt/eturnal/bin/eturnalctl info`